##HQ-CS-B

system-view

sysname HQ-CS-B

display current-configuration

interface Eth-Trunk 1

mode lacp-static

port link-type trunk

port trunk allow-pass vlan all

quit

interface GigabitEthernet 0/0/9

eth-trunk 1

quit

interface GigabitEthernet 0/0/10

eth-trunk 1

quit

vlan batch 4 5 200

interface Eth-Trunk 1

port trunk pvid vlan 200

quit

interface Vlanif 4

ip address 192.168.8.2 24

interface Vlanif 5

ip address 192.168.9.2 24

interface Vlanif 200

ip address 192.168.11.210 28

interface GigabitEthernet0/0/1

port link-type trunk

port trunk allow-pass vlan all

quit

interface GigabitEthernet0/0/2

port link-type trunk

port trunk allow-pass vlan all

quit

interface GigabitEthernet0/0/3

port link-type trunk

port trunk allow-pass vlan all

quit

vlan 20

interface GigabitEthernet0/0/3

port link-type access

port default vlan 20

quit

interface Vlanif 20

ip address 192.168.11.82 28

quit

ip route-static 0.0.0.0 0.0.0.0 10.0.11.83

quit

quit

//MSTP

stp region-configuration

region-name Huawei

instance 1 vlan 4

instance 1 vlan 5

active region-configuration

quit

stp instance 2 priority 4096

stp instance 1 priority 8192

//VRRP

interface Vlanif 4

vrrp vrid 1 virtual-ip 192.168.8.254

quit

interface Vlanif 5

vrrp vrid 2 virtual-ip 192.168.9.254

quit

interface LoopBack 0

ip address 192.168.11.130 28

quit

ospf 1 router-id 192.168.11.130

area 0

network 192.168.9.0 0.0.0.255

quit

quit