system-view

sysname HQ-R

//PPP :HQ-R& B1-R

interface serial 0/0/1

ip address 192.168.11.97 28

quit

interface serial 0/0/1

link-protocol hdlc

/y

quit

display interface Serial1/0/0

rip

version 2

network 192.168.0.0

quit

interface serial 0/0/1

link-protocol ppp

/y

quit

interface serial 0/0/1

ppp authentication-mode chap domain system

shutdown

quit

aaa

authentication-scheme system

authentication-mode local

quit

domain system

authentication-scheme system

quit

local-user user1@system password simple Huawei

local-user user1@system service-type ppp

quit

//FR:HQ-R& B2-R

interface serial 0/0/2

ip address 192.168.11.113 28

int loopback 0

ip address 192.168.11.131 28

quit

interface serial 0/0/2

link-protocol fr

/y

fr interface-type dce

fr dlci 102

quit

fr map ip 192.168.11.114 102 broadcast

undo summary

interface Serial 0/0/2

undo fr map ip 192.168.11.113 102

fr map ip 192.168.11.113 102

quit

//HQ-R& HQ-CS-A

Interface GigabitEthernet 0/0/0

ip address 192.168.11.66 28

//HQ-R& HQ-CS-B

Interface GigabitEthernet 0/0/1

ip address 192.168.11.82 28

ospf 1 router-id 192.168.11.131

area 0

network 192.168.12.0 0.0.0.255

network 192.168.13.0 0.0.0.255

network 192.168.14.0 0.0.0.255